	28 July 2017 

	Open House
	Let’s make it successful!
Confirm monitors with todd
Print out banner and grommet after lamintate
Update poster plots

	2018 proposal
	Submitted

	Current meter
	Go ahead with both. Collaborate with Drew about set them up. 1 with 4m range bends, 1 with 1 m range bends

	Core extruder
	Nov. Bring up in mid June

	Rover 
	Sharpen port chamber cam focus. The company can change the resistors/current of spare. Then we’ll swap the spare if it looks good in Nov.Submitted. Rotate those cameras 
10K lantern shark. Pressure tested when sent five years ago. Test it at sea. Remember in September/October.
Don’t need to get oil filled ducer. Try to contact Rover before picking up. If can’t contact on LF consider swapping 

	Sphere 
	Testing the one with a chip

	LED lighting-Brett
	Paul got them from Brett. Take 19 seconds to charge after sitting overnight. Takes 2 seconds to recharge after being fired….so capacitor bank not being used fully.

	Scanning QC
	RICH- can you help with renaming script? For us, yes
Danelle
Start trying it out

	Manuscripts
	1. Kathy’s multibeam Submitted 
2. Oceanography paper submitted

	Multibeam M
	This summer end of summer

	Personnel schedules
	Ken some time in September
Rich- 26 – 31 July



[bookmark: _GoBack] Purchasing: two more chain isolators

1. 50 ft of galvanized long-link chain (1/2”) and galvanized shackles (10 of 5/8” and 10 of ¾”) 
2. More 5 gallon white buckets- carry at least five with us. Check the van
3. More lugs and bolts for benthos releases
4. Buy more anodes. Make sure they are packed individually in plastic bags. – Send for quote for anodes and chain isolators
5. Oversize 11/16 carbite remer for camera tropod
6. Release o-rings- check sizes
7. More shoulder bushings for camera tripods
8. Better 37% formaldehyde and more borax to sea
9. Widemouth jars plastic UN certified
10. Second coring station
11. O rings for the current meter and isolation tape/heat shrink. Get same for Rover
For Pulse 69:
12. Iversen’s bio-op camera, then it goes into a gel.
13. Drill out all release anodes before we go to sea.
14. Both Knute and Marko are looking at how to release the tripod with the ROV if needed
15. Check releases for corrosion 
16. Modify drawing for SES depoymet
17. Argos beacon will go on Dualie
18. Which guts are in the RF beacon?
Crissy to add a spot for tripod strobe hard-hat SN on deploy checklist
19. Give bridge the RF freq so they can listen for sink time.
20. Get homers for both camera tripods from Conway
21. Add to deployment sheet which camera system it is
22. Troublshoot chamber optode from grab resp- check history of optode, cable
23. Chinese fingers on SES drop-weight
Misc
1. Rob Young- what do you really want?
2. Rob’s student (female) might come


End of year wish list:
Ti seaconns
Lasers
SES parts
