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	VARS
	UTC to Local

	2018 proposal
	Smarten SES?
Rigging for sampling at 600 m- 2018. Deploy at 50 mab in Nov
Spare sediment trap guts	
Frame with two releases, put them on end of mooring so can put on at any height
Pressure testing for one spare
VIPER- vertical integrated profiling event responder

	Fluorescence cams on tripod
	Budget for most expensive option…Proslica with stack. Is there room in FF camera housing? Possibly. Need main processor card with Ethernet, Newer version of Technologic. Maybe snappy can put that to sleepy-wakey. And light, deep sea power and light housing x 2. 2 bulkhead connectors/cables. 

	Wave glider
	Establish single point person for each team. Bother Brian after Canon

	Current meter
	Alana told them what memory to use

	Core extruder
	Nov. Bring up in mid June

	Sediment traps
	Spare guts- 6K tax and shipping for two sets. 6-8 weeks delivery time

	Rover 
	Sharpen port chamber cam focus. The company can change the resistors/current of spare. Then we’ll swap the spare if it looks good in Nov.Submitted. Rotate those cameras 
10K lantern shark. Pressure tested when sent five years ago. Test it at sea. Remember in September/October.
Don’t need to get oil filled ducer. Try to contact Rover before picking up. If can’t contact on LF consider swapping 

	LED lighting-Brett
	Brett and Paul still need to decide what to do with them

	Scanning QC
	RICH- can you help with renaming script? For us, yes
Danelle
Start trying it out

	Manuscripts
	1. Kathy’s multibeam paper- Submitted in next week
2. Feedback to Ken asap
3. Create drop box folder with images
4. Johnny to make image overlap fig in Solidworks

	Multibeam M
	This summer

	Jerseys
	Camo PULSE shirts. Stripe for each PULSE cruise. Full jumpers with tassels.  Eric will help with design

	Personnel schedules
	Crissy at cabin 18-25 May



 
 Dualie to do list
1. Both Knute and Marko are looking at how to release the tripod with the ROV if needed
2. Check releases for corrosion in Nov
3. Argos beacon will go on next time
4. Which guts are in the RF beacon 
5. Crissy to add a spot for tripod strobe hard-hat SN on deploy checklist
6. Need more freeweights. Get another full palette- Crissy
7. Give bridge the RF freq so they can listen for sink time.
8. O rings for the current meter and isolation tape/heat shrink. Get same for Rover
9. Get homers for both camera tripods from Conway
10. Add to deployment sheet which camera system it is
11. Spare sediment trap controllers
12. Chinese fingers on SES drop-weight
Monocam to do list
1. New weight emergency release so pilots can release mooring. Is pin system viable?
2. Aquarium fish nets for getting small stuff out of samplers
3. More 5 gallon white buckets- carry at least five with us. Check the van
4. Buy 50 ft of galvanized long-link chain (1/2”) and galvanized shackles (10 of 5/8” and 10 of ¾”) 
5. More lugs for benthos releases
6. Modify drawing for SES depoymet
7. Modify existing mast assembly replace the one on the dualie. Make a new top from the one that’s on the deck
8. Homers for dualie. Get two from Conway. 
9. Troublshoot chamber optode from grab resp- crissy to do
10. Wake up call to be more careful in rigging lines, especially in calm weather.
11. Oversize 11/16 carbite remer for camera tropod
12. Buy more anodes. Make sure they are packed individually in plastic bags. 
13. Drill out all release anodes before we go to sea.
14. Needs more bolts for acoustic releases
15. Release o-rings
16. More huge kim wipes
17. More shoulder bushings for camera tripods
18. Software for running current meter data. Try to look at it today. 
19. More falcon tubes
20. Widemouth jars plastic UN certified
21. Better 37% formaldehyde and more borax to sea
22. Second coring station
23. Two sets of top clamps for spar buoys
24. Ballast weights need four. 
25. Iversen’s bio-op camera, then it goes into a gel.
26. Rob Young- what do you really want?
27. Rob’s student (female) might come

