	18 December 2019

	Pulse 72 debrief
	ADCP download data- remove battery- Do today
All but SES images on pulse/project library
Go through tool boxes
Need to do a better job of cleaning isolator hardware
How will macro fit into this cruise?Give Diana a chance to do a replicate? Prioritize

	SES 
	Drilled out float bars so they will take the new shackles.
Wakey. There’s a limit to how many times you can write to the flash 
2 minute safety was in effect. Went through its scheduled 5000 sets.
Will Rover has an issue with this? Not likely.
John squeegies
Found some compatible brushes
Will go on to cable- check rover lab for connectors
Code for wakey

	Rover
	SCOC insertion depths
Chamber camera needs servicing- Remind in Jan
Johnny made new pivot pins, getting shinnied and will be done soon

	Tripod
	Red tagged mark I camera. Put a mark I back in.- Xif in late dec to see if camera had been used before.
Fresh coin cell in mark I but not dualie.
Update technical orders.

	Optodes
	Recalibrate and swap out.
Look for dip in rover reference during salp blooms
Check offset between reference optode readings Rover.
Rover optodes: Swap out one or two of the reference optodes. One is getting noisy
Can RBR logger work for a year so we can test the new optodes for a year

	ADCP postmordem
	Make mount for changing ADCP battery
Spare o-rings

	Year end spending
	Connectors- Alana spending $2k on Ti connector
Anodes, chain isolators- have plenty
Recalibrate all optodes and swap out 

	Lasers
	Dan came- recompile laser measure for matlab. He now has all the information and is processing info from the last dive. He wants to write a paper about it.
2 papers- one science one methods
No word

	Larvae pump
	Got MBARI board removed from Elmo. Serial number is not on there. Have RMA form.
Leaking filteration
All the bliss stuff is on pulse
Check battery- battery was 25.5. volts. Undischarged. Didn’t drain the battery through the fault.

	Macro system
(aka shrimpoteuthis)
	Trying to calculate how to angle the camera. Johnny trimming frame. 50 mm lens, higher contrast. Cut housing in half
Test in dark
In 2020 Change to easier to use menu? Engineering logging?
To measure angle off horizontal- ~30 degrees. Move to 45. Mount battery at mud level. 
1 meter between strobes
Deployment- how small can we make it?
Too big to take down on ROV. Can’t go on elevator with larval pump
No purge port, use alkalines for lasers
Pressure test? Pump helium in to test weld?
Playing with the angle

	Olmo
	Revising draft. Resolve field of view discrepancy . Paul working on it. 

	30 year volume
	8 accepted out of 16
Rest are in various stages of revision 

	[bookmark: _GoBack]Lab cleanup
	18 Dec. 

	Personnel schedules
	19-23 Dec Crissy in PA
Paul- dates 20 Dec – Jan 7th (Back on 8th)
Alana gone most of Christmas and New Years Weeks
Johnny taking off some time around Christmas
Ken is out New Years eve
Rich 23 Dec – Jan 2



