	30 October Sept 2019

	Pulse 72 debrief
	ADCP download data- remove battery
Paul focusing on laser measure, writing code
Lasers need to be taken off vehicle.
SES- timing
Larval sampler needs postmordem to see if water got into pump or index motor. Something blew up pump controller, main controller, main controller power supply.
Leaking filteration
Red tagged mark I camera. Put a mark I back in.- Xif in late dec to see if camera had been used before.
SCOC insertion depths
All but SES images on pulse/project library
Fresh coin cell in mark I but not dualie.
Update technical orders.
When johnny turnedaround dualie- reused release anodes from previous deployment. Once you crush the copper balls they can’t be reused.
Need to do a better job of cleaning isolator hardware
How will macro fit into this cruise?Give Diana a chance to do a replicate? Prioritize

	SES timing
	Wakey. There’s a limit to how many times you can write to the flash 
2 minute safety was in effect. Went through its scheduled 5000 sets.
Will Rover has an issue with this? Not likely.

	Optodes
	Recalibrate and swap out.
Look for dip in rover reference during salp blooms
Check offset between reference optode readings Rover

	Year end spending
	Camera
Connectors
Spare for macro
Anodes, chain isolators
We have 1 spare release
Optode
Recalibrate and swap out
Check offset between reference optode readings Rover

	Snappy delay
	Doesn’t work…working to figure it out. Mark III and IV issue.

	Lasers
	Hang up is mount. If we have angles, Johnny can make the mount. Working on getting the laser mount done.
Need to calibrate Tueday on shore. Ship gets back today 1900

	Upside down sediment trap
	Deployed.

	Larvae pump
	Need to post mortem.

	Macro system
(aka shrimpoteuthis)
	Don’t ask till after cruise
Sidelined until the other aspects are done. Keep up momemtum and finish after cruise.
50 mm lens, higher contrast. Cut housing in half
Will we have a pointer laser ready?
Lid’s coming in the mail.
Johnny working on endcap. 
Test in dark
In 2020 Change to easier to use menu? Engineering logging?
To measure angle off horizontal- ~30 degrees. Move to 45. Mount battery at mud level. 
No purge port, use alkalines for lasers
Pressure test? Pump helium in to test weld?

	Solo camera height, angles
	Not coming back. New mooring line will go on Solo camera and two inverted traps. 

	30 year volume
	Foram paper has been published

	Olmo
	Revising draft. Resolve field of view discrepancy 

	Personnel schedules
	Paul in texas- back Tuesday
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