	11 March 2020

	Lasers
	Use coral camera to hang target to test calibration software. Had to digitally remove red square. From that it can tell focal length and radial distortion of lens + port. Tells you principal point (center of radius of distortion).--Zhang paper
For 2020 aim for a paper, use this on animals
Support 2020 cruise (**test it on animals, 3D print a peniagone that won’t squish or turn to snot on the way up. see error based on “topography” of animal off the sea floor). 3 diff sizes, measure from head vs footprint?
Will show this to Dan Davis to incorporate it into Laser measure to make calibration more efficient. 5-10 min of bottom time.

	Loop and Cross
	Talked with Chris. WG going out next week. Paul will give est. Rover location.
Tom O’riley: We do this while we can test it in the bay.
Test it with any modem that we can hit. What other modems are out there?
Don’t wait till Station M to start testing, because of how finickey the modem connection is there.

	Rachel Carson 20-21 May
	Elevator with Larval pump deployed free vehicle.
Hydrophone drop off.
Deploy SES
Use the ROV to 
         Plug in SES
         make sure larval pump is working.
         Check on Quest
Weights need to be recovered. Otherwise have to get special permission from Sanctuary (if >500 lbs)
Precruise should go in soon. 

	SES 
	4 glass lenses coming. Ones off maching were scratched. Has been rubbing grit across the plates
Taken apart. Found leak in compensating diaphragm. We have three spare motors, two were leaking oil. 
Sent request for quote for 5 new diagrams. 
Refurb motors. Connect spare guts to SES. Let Rich do his magic.
Pull pin have it on the bottom
What happened to those floats that had been attached to SES frame when it was deployed at MARS? Castroville?
Ask Craig- is there a current meter out there?
Transissometer?
Still need board with all the diodes?
65 m of cables.
Work on squeegee. New slide. During wear test with 3 differrent durometers for squeegee. Use silicone.
Wakey. There’s a limit to how many times you can write to the flash 
Fluorescence reference in carousel add puck for monthly fluoro reference. Make sure glue isn’t fluorescence. Press it in.
Does the cloudiness happen at MARS? And if so, then will it clear faster?
Service all o-rings
Check front lit images
--Can we include an occasional image of a slide with a zero collect time?
Disassemble housigs to replace o-rings and plug in mars interface

	Rover
	Chamber camera needs servicing- keep reminding
Johnny made new pivot pins, still at plater
One chamber gives higher SCOC values than others.
Change out two chamber optodes. Take the two that we take off of it and see what the offsets are and can we correct for it?
Check LF ducer to modem

	Main Tripods
	Nothing to report

	Optodes
	Need boots for four optodes.
Swap out a couple.
Look for dip in rover reference during salp blooms
Is there a solution we should use in the field to rinse and get off any oils?
Check offset between reference optode readings Rover.
Rover optodes: Swap out one or two of the reference optodes. One is getting noisy
Can RBR logger work for a year so we can test the new optodes for a year

	CO2 sensor
	Meeting with Yui on 17 March, 1 pm Alana and Paul

	Larvae pump
	Failed its pressure test on fist cycle.
DJ sent part number of deep elmo oscillator. Paul ordered some. 
Will try one more time with new oscillator and better wiring done, and if that fails will make 1 atm housing. Johnny is looking into it.
If this other oscillator works then we don’t need to deal with al lot of complications.
Run only at depth, not on way down/up. ~2 hour descent. More than a day to get 4 cycles.
Base plate of the power filter board- stripped
Design housing, or buy pressure-tested housing? 
Tuned with long time constant to avoind voltage spikes from abrubt stop.
Titanium servo like on Rover? That’s plan B if pressure test fails.
Instead of jeopardizing insert, use old cable. Old 8 pin whip. 
Apparently the whole assembly had never been tested at 4000 m. Now going to test the whole thing.
After test clean pump and “meger” it.
Dale may have a whistle we can use.

Leaking filteration
Needs a schematic given to Paul so he can rewire the thruster backup. Dale;s and Alana has access to it.

	Macro system
(aka shrimpoteuthis)
	Johnny making chassis- cut, machine, welded
Put 50 mm lens on, put in pocket of face plate and it fits. There’s a teeny tiny bit of shadow on the bottom corners but it’s fine.
Rough estimate of 35 degrees of it looking down but bottom bar might be in view. Don’t want to cantilever the camera out
Johnny to model parts before cutting the housing.
In 2020 Change to easier to use menu? Engineering logging?
Mount battery at mud level. 
1 meter between strobes
Deployment- how small can we make it?
No purge port, use alkalines for lasers
Pressure test? Pump helium in to test weld?
Macro aiming laser
Test in July
1 Min-K10 ccpl-ti- Alana owes us.
More time mid march

	Snappy
	Success. It’s in project library. 1.35
Newer compiler blows storage budget. Spits out so much.
Paul built new version, but code base wakey, snappy compiler no longer compiles.
Have to get an recompile all of our code bases. 
Microchip compiler Paul to look at, and will call in pro. 

	Sediment trap samples
	Sorting, splitting

	Olmo
	In review 

	Personnel schedules
	Crissy- April ~ 1-11?
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	Loans
	Alana replaced titanium connector and min-k 




