MBARI Ventana Camera Cable wiring diagram.
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RG-179, Video Core

Dark Blue 22 gage     (of dark Blue - Green twisted pair)

Cable Foil Shield - Drain Wire

Green 22 gage       (of dark Blue - Green Twisted pair)

White 22 gage (of white - grey twisted pair)

Lt. Blue 20 gage + RG-179 Video Shield

Red 22 gage

Grey 22 gage (of white - grey twisted pair)

Yel 22 gage

pin 3 has two connections, Lt. Blue 20 gage and RG-179 video Shield

Both Ends are terminated with MIN-K-10's, the exact length is not important, both cables should be approximately 12 feet.

Orange 20 gage

Rx 232/485

Tx 232/485

Spare

Power and Video Ground

12 VDC

24 VDC

Video Core

Spare - Video Sync

spare

Cable shield - earth ground

dark blue polyeurythane Cable has nominal diameter of .370 inches - two 12.5 feet pieces are supplied via CF#10745


Contact information:  DJ Osborne, MBARI  831 775 1908  phone,   831 775 1652 fax

