FOCE Chassis Power Supply Board 

Software:
Simple command structure to/from chassis CPU Board

Interface:
Backplane SPI bus (dedicated CS?)
RS-485

Supplies:
3.3Vdc @ 8A max (26.4W)
5.0Vdc @ 4A max (20W)
12.0Vdc @ 2A max (24W)

Input Voltage:
24Vdc 

Features:
Dedicated slot address
Current/voltage monitoring for all inputs/outputs
Separate outputs for 7.5Vdc? (Netgear)  (or 2-3 adjustable outputs?)
System level 3.3Vdc (Always on)
Voltage references(?)
Onboard PIC
DC-DC Converters sync’d together
DC-DC Converters can be powered down via XPort on CPU Board


