


Event log from Sunday April 10, 2011

08:31  - stopMotorCycle
08:34 - rmotor loc ESWpump md;
08:36 -  rmotor loc /dev/ttyS8 md;
	rmotor loc /dev/ttyS10 md;

08:40 - GUI: Turned off both motors. Turned off all 3 cameras, turned off all 3 LEDs.
08:41 - Turned off pH probes 1-5. Turned off ADCP and ADV.
08:42 - Turned off both CTDs.

08:43 [STATUS] - pH6 On, CO2 On, All Cameras, LEDs off.

09:45 - shutdownPort loc CO2subsys
09:47 GUI: Turned off CO2subsys and Valve Assy

10:44 Computer locked up - Had to pull battery/reboot

10:52 Restarted GUI and Turned on Forward LED.

11:50 GUI: Turned off Fwd LED, turned on Center LED

12:54 Had to restart GUI. GUI: Turned off Center LED, turned on Aft LED

13:52 GUI: Turned off Aft LED, turned on Forward Camera

14:50 GUI: Turned off Fwd Camera, turned on center camera

15:49 GUI: Turned off Center Cam, Turned on Aft camera

16:50 GUI: Turned off Aft camera
16:54 GUI: Turned on CO2 Subsys
16:56 scanPort loc /dev/ttyS9 (ADCP)
16:57 GUI: Turned off CO2 subsys

18:30 scanPort loc /dev/ttyS4 (CTD1)

19:32 shutdownPort loc /dev/ttyS4
	scanPort loc /dev/ttyS6 (CTD2)

20:33 shutdownPort loc /dev/ttyS6
	scanPort loc /dev/ttyS11 (ADV)


21:32 shutdownPort loc /dev/ttyS11
	scanPort loc /dev/ttyS8 (Mot1)

22:51 shutdownPort loc /dev/ttyS8


