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	1. Ensure that dovekie is configured to run onboard the Zephyr

· % sudo /operations/config.ship (use doroado1 as pwd)
2. Check dovekie environment is correct

· % source ~/st4/TREX/devConfig

· % env|grep TREX to double check
3. Check mvc-dmo1 is up and visible 

· % ping mvc-dmo1

4. Ensure trex2 on AUV is up

· % telnet mvc-dmo1 (dorado1/dorado1)

· % cd auv_autonomy

· % source configSrc

· % env| grep AUV to double check
· % qtalk –m /dev/ser13

· !a <ENTER> // To turn on trex2 [!f <ENTER> // To turn off]

· ^a to exit qtalk
5. Check that on trex2 the correct MVC-VCS port is being pointed to:

· % cd ~/amc/missions/

· % cat vcs.cfg

i. it should show port # 8002 and remotemachine as mvc-dmo1
· check analogously on mvc-dmo1 that this port is also referenced

i. % cat $AUV_CONFIG_DIR/statePublisher.cfg should shows the same port #

6. Check that trex2 has the right safety behaviors configured:

· % cd amc/missions

· % cat init.cfg

7. Check that mvc-dmo1 

· has the right $AUV* environment variables pointing to ~/auv_autonomy
· port and IP for trex2
i. % cat $AUV_CONFIG_DIR/statePublisher.cfg shows

1. AMC_IP is set to 134.89.32.39

ii. ClusterName is set to plume

· abort plan 

i. % cat $AUV/missions/abortMPlan.cfg

· cluster configuration files

i. % cd $AUV/bin

ii. % make install_cfg (this will install the operational cluster conf)
iii. % make install_sim_cfg (this will install the sim cluster conf)

· check auv_autonomy code base was updated and current from auv head

i. % cvs –n update (on dovekie)

8. Check binary image sizes (26087 bytes) and checksums on 

· dovekie: ~dorado1/st4/TREX/ctd2007/amc_o_rt

· trex2:~dorado1/amc/exec/amc_o_rt
9. Before the AUV is in the water and on the deck, configure dovekie to talk to trex2 via the Freewave modem

· % /operations/config.freewave
10. Ensure mvc-dmo1 can also be reached

· % ping mvc-dmo1
11. When firing up the amc for mission start, ensure nohup command

· %  nohup amc_o_rt <mission config file> &
Tip:

a When moving dovekie between networks one should do
· % /etc/init.d/network stop

· % /etc/init.d/network start




