ROV (NAME TBD)
General Summary
Specifications:

Depth rating  = 4000 meters

Vehicle Type = Electro/Hydraulic

Vehicle Power = 75shp

Vertical Thrust > 550kg
Horizontal Thrust > 650kg
Variable Buoyancy System = 135kg
Hydraulic Systems and Components

· 7 function 15 lpm hyd. solenoid valve pack w/flow controls (on Tool skids)

· 12 function auxiliary valve pack 

· (8) 15 lpm solenoid valves

· (4) 8 lpm proportional valves with remote flow control

· Spare HP (30 lpm) bi-directional tooling port

Science Payload = 275kg (in water weight) in addition to the below listed equipment and tool skids
Auxiliary Instrument Power & available voltages
· ~8kW

· 240, 48, 24, 12, 5 VDC

· 110 VAC

Auxiliary Video & Data

· (2) spare single mode fibers

· (1)100bt Ethernet port

· (1)10bt Ethernet port

· (10) RS-232 serial ports (expandable if required)

· (4) RS-485 serial ports (expandable if required)

· (7) Video channels

Core Navigation Instrumentation

· RDI – Workhorse Navigator DVL (1.2mHz)

· Octans 6000m FOG (primary heading reference)

· Tritech FOG (secondary heading reference)

· Paroscientific depth sensor

· Mesotech Altimeter

· Mesotech 1071 scanning sonar

· Sonardyne ROV Homer

· Sonardyne Fusion USBL

Core Science Tools and Instrumentation

· Benthic tool skid (standard configuration)
· Suction sampler w/12 bucket carousel

· Swing arm

· Sample drawer

· (24) tube cores

· Mid-water tool skid (standard configuration)
· Suction sampler w/12 bucket carousel

· (2) Swing arms

· (6) Detritus samplers

· 4km cable laying tool skid

· Schilling T2 7 function manipulator

· Kraft Raptor 7 function manipulator w/force feedback

· CTD w/transmissometer

Core Cameras & Viewing Tools

· (2) ROS PT-25 pan & tilts

· (2) ROS PT-10 pan & tilts

· Insite Triton HDTV camera w/10x zoom (Science)
· 3 chip/750 line – wide angle - color camera (Pilot navigation)

· Digital still camera & strobe

· Internal pan & tilt color camera w/zoom (down looks front viewing area)

Lighting

· (6) 400 watt HMI lights

· (4) 250 watt Incandescent lights

Umbilical 
· .68”(17.5mm) OD.
· (5) single mode fibers

· (5) power cores

ROV Auto Functions

· Auto Depth

· Auto Heading

· Auto Altitude

· Auto Hold (Dynamic Station Keep)

· Auto Step (X, Y and Z)

· Auto Home

· Auto Track (Cable & pipe tracking)

· Auto Route (Follows a pre-programmed route of waypoints)

· Auto Lost Thruster Compensation

· Auto Pitch & Roll trim

