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 Thursday, March 22, 2007

QUOTE

(1) PK50002MA   
Crane Power / Palfinger Marine fully hydraulic foldable marine crane 

· Maximum lifting moment 48,7 mt

· Classification according to LRS Code for Lifting Appliances - Shipboard Cranes

· Hydraulic outreach 7,7 m  (2-section hydraulic boom extension)

· Overall dimensions acc. to data sheet 

· Lifting capacities PK50002MA acc. to data sheet 

· Continuous slewing

· Net slewing moment maximum 7,0 mt

· Special crane base of cylindrical design for minimum space requirement

· Marine version ball bearing slewing ring

· Standing platform on crane column

· Special protection against corrosion for piston rods and pins

· Danfoss marine specification control valve mounted at the standing platform

· Fully hydraulic working overload cut-off system

· Load holding valves on slewing, inner, outer and extension boom cylinders

· High pressure filter

· Stainless steel hose and pipe fittings, metric acc. to DIN2353

· Stainless steel hydraulic pipes

· Stainless steel pipe clamps

· All Crane Power / Palfinger Marine fitted bolts and nuts (except mounting bolts - dacrometized) are stainless steel

· All steel components grit blasted SA2.5 acc. DIN EN ISO12944

· Special seawater resistant 3-layer marine paint finish, blue RAL 5013,

· Minimum total dry thickness 210 micron 

· Mounting bolts and accessory according to data sheet

· Attachment: spare can of finish paint (packed in attachment case) 

· 2 set of technical documentation:

· Crane Power / Palfinger Marine test certificate including 25% static overload test for the crane

· Operator’s manual in English and German language

· Spare parts list in English and German language

· Instructions for installation

· Hydraulic diagram

· Maximum operating pressure acc. to hydraulic diagram

· Recommended oil flow acc. to hydraulic diagram

Total amount









$ 126,378.00

M0625
Mounting base, height 0,5 m, 50µm dry thickness primary painting
$     3,575.00

VERP1
 Crating: crane on pallet, attachments packed in cases


$        572.00

TERMS: 

· 50% due upon order
· Balance payable upon completion at PHE and before final shipment to customer. 
· Price are FOB Factory in Slovenia
· All prices are valid for 30 days
· All prices are in US dollars
