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Brett Hobson
Mechanical Engineer
Monterey Bay Aquarium Research Institute
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(831) 775-1941
hobson@mbari.org
QUOTE

(1) PK65002MA    Crane Power / Palfinger Marine fully hydraulic foldable marine crane 

· Max. Lifting moment 61,4 mt 
· Classification according to LRS Code for Lifting Appliances - Shipboard Cranes

· Hydraulic outreach  7,7 m  (2-section hydraulic boom extension) = 25 ft (aprox)
· Overall dimensions according to data sheet 
· Lifting capacities PK65002MA @ 4,351 PSI

· 28,660 lbs @  15 ft

· 22,046 lbs @ 19.5 ft

· 17,637 lbs @ 25 ft (full reach)

· Please note the above capacities are not at the de-rated state. 

· For 4000 PSI, capacities would be de-rated approximately 8%.  At this pressure, the crane meets your requirement. 
· Continuous slewing

· Net slewing moment max. 7,0 mt

· Special crane base of cylindrical design for minimum space requirement

· Marine version ball bearing slewing ring

· Standing platform on crane column

· Special protection against corrosion for piston rods and pins

· Danfoss marine specification control valve mounted at the standing platform

· Fully hydraulic working overload cut-off system

· Load holding valves on slewing, inner, outer and extension boom cylinders

· High pressure filter

· Stainless steel hose and pipe fittings, metric acc. To DIN2353

· Stainless steel hydraulic pipes

· Stainless steel pipe clamps

· All Crane Power / Palfinger Marine fitted bolts and nuts (except mounting bolts - dacrometized)

· Are stainless steel

· All steel components grit blasted SA2.5 acc. DIN EN ISO12944

· Special seawater resistant 3-layer marine paint finish, blue RAL 5013,

· Minimum total dry thickness 210 micron

· Mounting bolts and accessory  acc. To data sheet 

· Attachment: spare can of finish paint (packed in attachment case)

· 1 set of technical documentation:

· Crane Power / Palfinger Marine test certificate including 25% static overload test for the crane

· Operators manual in English
· Spare parts list in English
· Instructions for installation

· Hydraulic diagram 

· Max. Operating pressure acc. to hydraulic Diagram

· Recommended oil flow acc. to hydraulic Diagram

Total amount








$ 172,746.00
M0625
Mounting base, height 0,5 m, 50µm dry thickness primary painting
$     3,948.00
VERP1
 Crating: crane on pallet, attachments packed in cases


$        630.00

TERMS: 

· 50% due upon order
· Balance payable upon completion at PHE and before final shipment to customer. 
· Price are FOB Factory in Slovenia
· Availability: 28—20 weeks (Plus sea freight)
· All prices are valid for 30 days
· All prices are in US dollars
