Tiburon II Instrument Configurations
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1. DVL

String Format:

PD5

String Example:
See manual
String frequency:
Variable, see manual
Polled/Streaming:
Streaming

Serial Settings:
9600 8N1

Comments:


2. Digiquartz

String Format:

Standard output, see manual
String Example:
See manual

String frequency:
<TBD>

Polled/Streaming:
Streaming

Serial Settings:
9600 8N1

Comments:



3. Altimeter
String Format:

<TBD>
String Example:
<TBD>


String frequency:
<TBD>


Polled/Streaming:
<TBD>


Serial Settings:
<TBD>

Comments:
4. Octans Gyro

String Format:

TMS CCV IMBAT
String Example:
See manual

String frequency:
10 Hz
Polled/Streaming:
Streaming

Serial Settings:
9600 8N1

Comments:



5. iGC gyro

String Format:

<TBD>
String Example:
<TBD>
String frequency:
<TBD>

Polled/Streaming:
<TBD>
Serial Settings:
<TBD>
Comments:

MBARI is not planning on using the iGC gyro data so whatever configuration SMD chooses is acceptable.
6. Umbilical data
String Format:

$NVP string, see “Tiburon II External Device Data Format.doc”

String Example:
See “Tiburon II External Device Data Format.doc”
String frequency:
10 Hz
Polled/Streaming:
Streaming

Serial Settings:
38400 8N1

Comments:



