MBARI Test Software Setup Instructions

The following steps should get you up and running with the test software. This software is a cut down version of one of our QX series ROVs that you can use to learn about configuration, screen design etc. If you need any help drop me a line at

martin.jackson@smdhydrovision.com
Install Microsoft Virtual Machine 2007 on PC (free download from Microsoft)
Copy VM directory (MBARI4 or MBARI5) to root directory of PC

Run setup wizard in VM and add ‘existing’ setup MBARI4 (Node 4 – co-pilot display) for first PC/Laptop. Repeat for second PC/Laptop MBARI5 (Node 5 – touch screen) you don’t need a touch screen, as you can just use mouse to control the display. PCs should be networked to ‘see’ each other.
When the PCs boot up they automatically run the control system, to escape to QNX shell (to examine setup files etc.) press and hold [CTRL][ALT][SHIFT] then press [BACK SPACE]. TO login to QNX username: root

I am preparing some notes to assist in understanding system configuration, but these are not ready yet …

Best regards
Martin Jackson

Control Engineer

SMD Hydrovision
