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Tank Test Two - Plan
Assumptions:

1. The motherboard IS present.  
2. The load controller boards are NOT present.  A temporary wiring harness supplies power directly to the necessary instruments
3. The vehicle is fully assembled excluding the drop weight and the propeller.
Dry Lab Tests
Measure the motor efficiency with the dynamometer.  Take data at 90, 150 and 300 rpm for the following cases:

1. No load.
2. Expected load for the vehicle flying (see Yanwu’s e-mail).
3. Bollard; 30.6, 85.0 and 340 mNm respectively.
Assemble the vehicle, excluding the propeller and the drop weight.   Put tape (spiral pattern) on the propeller shaft to aid visual detection of rotation.
1. Test (dry) Freewave modem in the lab, using the new antenna.
2. Disconnect the tether, verify that the CPU boots up and runs normally on battery power.  Perform all the following tests on battery power without the umbilical.

3. Test rudder and elevator motion and range.  Verify that they move through the full range without binding when commanded by the operator.

4. Re-verify open-loop battery motion and VB operation after closing the vehicle.

5. Re-verify motor and shaft operation with the vehicle closed and dry.

6. Roll the vehicle out on the back deck.  Test GPS and Ir with the new antenna. Start Argos transmitter, and check for email fixes after dry tests are complete.
7. Roll the vehicle out into the parking lot.  Perform the Spartan compass calibration.  Try spinning the motor to see if the compass reading is affected.

8. Verify Spartan operation; compass and tilt.  Start a short mission, move the vehicle (in the cradle) in heading and pitch, then download the slate over the Freewave and plot with it with Matlab.

9. Verify negative-feedback control of heading and pitch.   Start a short setpoint or depth mission, move vehicle horizontally and then vertically in the cradle and verify that the rudder and elevator moves in the opposite direction. Plot the data with Matlab and Google Earth. (Rob)

10. Test the manual weight drop feature.  Issue the command, then verify that the burn wire has the correct voltage applied.

11. Test emergency board operation.  Start a mission, then kill the flight code (the “ap”).  Verify that the code restarts.  Kill it repeatedly, creating a situation where the emergency board should activate.  Verify that the dropweight burn wire subsequently has voltage applied, and that the GPS, Ir, and Freewave come on as planned.  See the emergency board flow chart.
12. Suspend Argos transmissions

Tank Tests
1. Pump 1/3 of the oil (333 ml) outside of the housing with the vehicle dry, using the Freewave.  Put the vehicle in the tank, then ballast neutral and trim level without the umbilical. (Thomas)
2. Pump the oil fully out for maximum buoyancy. With the vehicle free floating in the tank, verify that the Freewave works. Test data transfer and note data rate.  Check vehicle roll angle, stability and antenna height. (Possibly log Ahrs)
3. Pump oil into the vehicle and adjust vehicle pitch (move batt.) to determine minimum buoyancy needed to hole antenna aloft. 
4. Plug in the umbilical; re-verify wet umbilical operation.

5. Test the CTD depth sensor with the umbilical attached.  Pump the vehicle negative, lower it to various depths, verify that the depth sensor output changes and reads correctly.  
6. With the vehicle still negative, then run a constant-depth mission (prop not attached, but shaft spinning) while manually lowering the vehicle below, than raising it above the setpoint.   Verify that the elevators always turn to oppose the depth error.
7. Lower the vehicle below the abort depth and verify the prop shuts off.

8. Test drop weight burn wire.  Use a weight bag, secured by a line, to drop when the wire burns.

9. Measure the power consumed by the motor at 90, 150 and 300 rpm (prop still not attached), vehicle submerged.  We’ll subtract the bench no-load power measurement from this to get a drivetrain efficiency (water windage loss) number.
10. Pump the oil back to neutral buoyancy.  Disconnect the umbilical.  Run a mission that moves battery to full forward and aft positions with the vehicle adrift in the tank, except for a tag line.  Check vehicle pitch by plotting logged data.  
11. Repeat item 6 with the umbilical still disconnected.  Verify that when the vehicle is raised to within 1 meter of the surface (surface threshold) the code pumps the oil completely out for maximum buoyancy.
12. Suspend vehicle from fish scale.  Set buoyancy fully negative (about 3.3 N).   
a. Measure weight just below the surface.

b. Estimate entrained air by comparing weight at 9m depth.
Harbor Tests

1. Reverify the GPS and Iridium operation, with the vehicle in the cradle, outside on the dock. 
2. Test the Argos system.  Confirm there are satellites in view with JPASS.
3. Put the vehicle in the (harbor) water and repeat the above tests.  Try moving the Freewave base further away to verify that it has sufficient range.  Verify that GPS and Ir still work in the water.
4. Repeat the emergency board test (Dry Lab, Item 11), with the vehicle still in the water.  Verify that when the flight code is repeatedly killed, the Ir activates in emergency mode and that SBD messages are received and contain the correct Gps location.

Tasks Deferred to TT3
1. Test the Dvl

2. Test altitude abort using the Dvl altimeter.
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