Vehicle Close Out Check List
1. Motherboard

a. Board serial number #2 TTH
b. Vehicle Name is “Tethys” TTH
c. Memory Card Installed? Yes, 8GB TTH
d. LED Jumpers

	Jumper
	Comment
	Status (1 = On)
	Removed

	26
	24 vdc LC
	1
	√ TTH

	32
	5 vdc 
	1
	√ TTH

	33
	3.3 vdc
	1
	√ TTH

	31
	3.15 vdc
	1
	√ TTH

	36
	12 vdc LC
	1
	√ TTH

	35
	5 vdc LC
	1
	√ TTH

	34
	3.3 vdc LC
	1
	√ TTH

	41
	Shore Power
	0
	√ TTH

	43
	1.8 vdc
	1
	√ TTH

	30
	Vehicle Power
	1
	√ TTH

	42
	Battery Power
	1
	√ TTH


e. Connectors
	Connector
	Description
	Plugged in (Y/N)

	J-3
	?
	N √ TTH

	J-4
	Batt comms
	Y √ TTH

	J-5
	485 comms EZ servo
	Y √ TTH

	J-6
	SP3004D
	Y √ TTH

	J-7
	Iridium
	Y √ TTH

	J-8
	Batt comms
	Y √ TTH

	J-9
	H2O detect
	Y √ TTH

	J-10
	H2O detect
	Y √ TTH

	J-11
	Humidity and Temp
	Y √ TTH

	J-12
	Jumper
	Y √ TTH

	J-13
	Jumper
	Y √ TTH

	J-14
	Sea water ground
	Y √ TTH

	J-20
	Drop weight / burn wire
	Y √ TTH

	J-21
	Iridium power
	Y √ TTH

	J-23
	Ethernet
	Y √ TTH

	J-31
	?
	N √ TTH

	J-32
	DVL
	Y √ TTH

	J-33
	Free Wave
	Y √ TTH

	J-34
	Tether
	Y √ TTH

	J-35
	Main Batt
	Y √ TTH

	J-36
	Aux
	N √ TTH

	J-37
	Emerg Batt
	Y √ TTH

	J-38
	Slot 1 LCB #0
	Y √ TTH

	J-39
	Slot 2 LCB #0
	Y √ TTH

	J-40
	Freewave power
	Y √ TTH

	J-46
	LCB #2 SPI
	Res 13-15  √ TTH

	J-47
	LCB #2 power
	N √ TTH

	J-48
	LCB #1 power
	N √ TTH

	J-49
	LCB #0 power
	Y √ TTH

	J-50
	LCB #1 SPI (single wire?)
	Y √ TTH

	J-51
	LCB #0 SPI
	Y √ TTH


2. EZ Servos
	Name
	Address
	J-1
	J-2
	J-3
	J-4
	J-5
	J-6
	Checked?

	Elevator
	1
	-
	Y
	-
	-
	Y
	Y
	√ TTH

	Rudder
	2
	-
	Y
	-
	-
	Y
	Y
	√ TTH

	Prop
	3
	-
	Y
	Y
	Y
	-
	Y
	√ TTH

	VB
	6
	Y
	Y
	Y
	Y
	Y
	Y
	√ TTH

	Mass Shifter
	4
	-
	Y
	-
	Y
	Y
	Y
	√ TTH


3. Variable Buoyancy Valve Board

	Connector
	Connected?

	Shutoff Valve
	Y √ TTH

	Pressure Switch
	Y √ TTH

	VB EZSV23
	Y √ TTH

	Batt Pwr
	Y √ TTH


a. Pressure switch set at 100 psig √ TTH

4. Shore Power DEMUX-MUX boards

a. DEMUX  √ TTH

i. Two supply connections on positive board

ii. One load connection on positive boar

iii. Two supply connections on negative board

iv. One load connection on negative board

v. Sense lines connected to positive and negative posts

b. MUX  √ TTH

i. One positive connection

ii. One negative connection

iii. Six load connections to Ocean Servers

5. Battery Boards  √ TTH
a. All connectors are verified installed and tight

6. Emergency Battery  √ TTH
a. Installed (open circuit) 12.60 vdc

b. New on 12/1/2009

7. Mass Shifter stops  √ TTH
a. Aft at 9 5/8 inches

b. Fwd at 37 5/8 inches

8. Iridium  √ TTH
a. coI

b. tNe

9. Internal transponder batteries NOT installed. √ TTH

10. Weights Installed  √ TTH
a. Forward

i. None

b. Aft

i. None

11. Clean and inspect aft dome o-rings  √ TTH
12. Clean and inspect fwd dome o-rings  √ TTH
13. clean and inspect bolt o-rings  √ TTH
14. Install 20 new desiccant bags  √ TTH
15. Install PV tube  √ TTH
a. Verify water detect sensors touching inside surface of tube

b. Verify all internal wires are clear

c. Verify o-rings seat

16. Install Forward Dome  √ TTH
a. Make Amphenol connection

b. Torque bolts to 75 inch pounds

17. Draw vacuum

a. 7.5 inches Hg at 1200 01/21/2010

