Vehicle Close Out Check List
1. Motherboard

a. Board serial number #1

b. Vehicle Name is “Melia”

c. Memory Card Installed

d. Connectors
	Connector
	Plugged in (Y/N)
	Comment

	J-23
	Y
	Ethernet

	J-33
	Y
	Free Wave

	J-32
	Y
	DVL

	J-4
	Y
	Batt comms

	J-5
	Y
	485 comms EZ servo

	J-6
	Y
	SP3004D

	J-7
	Y
	Iridium

	J-8
	Y
	Batt comms

	J-14
	Y
	Ground?

	J-51
	Y
	LCB #0

	J-50
	Y
	Single wire?

	J-49
	Y
	LCB #0

	J-37
	Y
	Emg Batt

	J-35
	Y
	Main Batt

	J-36
	Y
	Shore Power

	J-38
	Y
	Slot 1 LCB #0

	J-39
	Y
	Slot 2 LCB #0

	J-20
	Y
	Drop weight / burn wire

	J-9
	Y
	H2O detect

	J-10
	Y
	H2O detect

	J-12
	Y
	Jumper

	J-13
	Y
	Jumper

	J-11
	Y
	Humidity and Temp

	J-21
	Y
	Iridium power

	J-40
	Y
	Freewave power

	TP-70 / TP-55
	Y
	Volt sense lines


2. EZ Servos
	Name
	Address
	J-1
	J-2
	J-3
	J-4
	J-5
	J-6

	Elevator
	1
	-
	Y
	-
	-
	Y
	Y

	Rudder
	2
	-
	Y
	-
	-
	Y
	Y

	Prop
	3
	-
	Y
	Y
	Y
	-
	Y

	VB
	6
	Y
	Y
	Y
	Y
	Y
	Y

	Mass Shifter
	4
	-
	Y
	-
	Y
	Y
	Y


3. Emergency Battery

a. Open circuit 12.82vdc, 

b. Installed 12.82 vdc

c. New on 12/1/2009

4. Mass Shifter stops
a. Aft at 9 5/8 inches

b. Fwd at 37 5/8 inches

5. Iridium

a. coI

b. tNe

6. Weights Installed
a. Forward

i. None

b. Aft

i. None

7. Clean and inspect aft dome o-rings

8. Clean and inspect fwd dome o-rings

9. clean and inspect bolt o-rings

10. Install 12 new dessicant bags

11. Install PV tube

a. Verify water detect sensors touching inside surface of tube

b. Verify all internal wires are clear

c. Verify o-rings seat

12. Install Forward Dome

a. Make amphenol connection

b. Torque bolts to 75 inch pounds

13. Draw vacuum

a. 15 inches Hg at 1800 01/05/2010

