Vehicle Close Out Check List

1. Motherboard

a. Board serial number #2 

b. Vehicle Name is “Tethys” 

c. Memory Card Installed? 

d. LED Jumpers

	Jumper
	Comment
	Status (1 = On)
	Removed?

	JP-26
	24 vdc LC
	1
	TTH

	JP-32
	5 vdc 
	1
	TTH

	JP-33
	3.3 vdc
	1
	TTH

	JP-31
	3.15 vdc
	1
	TTH

	JP-36
	12 vdc LC
	1
	TTH

	JP-35
	5 vdc LC
	1
	TTH

	JP-34
	3.3 vdc LC
	1
	TTH

	JP-41
	Shore Power
	0
	TTH

	JP-43
	1.8 vdc
	1
	TTH

	JP-30
	Vehicle Power
	1
	TTH

	JP-42
	Battery Power
	1
	TTH


e. Other Jumpers

	Jumper
	Comment
	Status
	Correct?

	JP-12
	
	3&4 7&8
	

	JP-13
	
	3&4 7&8
	

	JP-20
	
	3&4 7&8
	

	JP-8
	UART 1
	3&4 7&8
	

	JP-9
	1&2, 5&6
	1&2, 5&6
	

	JP-10
	UART 3
	Open
	

	JP-11
	
	3&4 7&8
	

	JP-14
	
	3&4 7&8
	

	JP-18
	
	1&2 5&6
	

	JP-16
	
	3&4 7&8
	

	JP-21
	
	1&2
	

	JP-23
	
	1&2
	

	JP-15
	
	1&2
	

	JP-17
	
	1&2
	

	JP-19
	
	1&2
	

	JP-37
	
	3&4
	

	JP-40
	
	open
	

	JP-2
	
	open
	

	JP-4
	
	open
	

	JP-22
	
	1 & 2
	

	JP-27
	
	open
	


f. Connectors

	Connector
	Description
	Correct?

	J-3
	!! empty !!
	

	J-4
	Batt comms
	 

	J-5
	485 comms EZ servo
	 

	J-6
	SP3004D
	 

	J-7
	Iridium
	 

	J-8
	Batt comms
	 

	J-9
	H2O detect
	 

	J-10
	H2O detect
	 

	J-11
	Humidity and Temp
	 

	J-14
	Sea water ground
	 

	J-20
	Drop weight / burn wire
	

	J-21
	Iridium power
	 

	J-23
	Ethernet
	 

	J-31
	!! empty !!
	 

	J-32
	DVL
	 

	J-33
	Free Wave
	 

	J-34
	Tether
	 

	J-35
	Main Batt
	 

	J-36
	Shore Power !! empty !!
	 

	J-37
	Emerg Batt
	 

	J-38
	Slot 1 LCB #0
	 

	J-39
	Slot 2 LCB #0
	 

	J-40
	Freewave power
	 

	J-46
	LCB #2 SPI !! Res 13-15 !!
	  

	J-47
	LCB #2 power
	 

	J-48
	LCB #1 power
	 

	J-49
	LCB #0 power
	 

	J-50
	LCB #1 SPI !! Res 13-15 !!
	 

	J-51
	LCB #0 SPI
	 


2. EZ Servos

	Name
	Address
	J-1
	J-2
	J-3
	J-4
	J-5
	J-6
	Checked?

	Elevator
	1
	-
	
	-
	-
	
	
	

	Rudder
	2
	-
	
	-
	-
	
	
	

	Prop
	3
	-
	
	
	
	-
	
	

	VB
	6
	
	
	
	
	
	
	

	Mass Shifter
	4
	-
	
	-
	
	
	
	


3. Variable Buoyancy Valve Board

	Connector
	Connected?

	Shutoff Valve
	 

	Pressure Switch
	 

	VB EZSV23
	 

	Batt Pwr
	 


a. Pressure switch set at 100 psig 

4. Shore Power DEMUX-MUX boards

a. DEMUX  

i. Two supply connections on positive board

ii. One load connection on positive boar

iii. Two supply connections on negative board

iv. One load connection on negative board

v. Sense lines connected to positive and negative posts

b. MUX  

i. One positive connection

ii. One negative connection

iii. Six load connections to Ocean Servers

5. Battery Boards  

a. All connectors are verified installed and tight

6. Emergency Battery  

a. Voltage: _____________

b. New on ______/______/_________

7. Mass Shifter stops  

a. Aft at 9 5/8 inches

b. Fwd at 37 5/8 inches

8. Iridium  

a. coI

b. tNe

9. Internal transponder batteries NOT installed. 

10. Weights Installed  

a. Forward

i. None

b. Aft

i. None

11. Clean and inspect aft dome o-rings  

12. Clean and inspect fwd dome o-rings  

13. clean and inspect bolt o-rings  

14. Install 20 new desiccant bags  

15. Install PV tube  

a. Verify water detect sensors touching inside surface of tube

b. Verify all internal wires are clear

c. Verify o-rings seat

16. Install Forward Dome  

a. Make Amphenol connection

b. Torque bolts to 75 inch pounds

17. Draw vacuum

a. ____ inches Hg  / ____ psi    at _______________

