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cisco RV082 10/100 8-Port VPN Router
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You can get I settings assigned automaticaly i your network supports
this capabiity. Otherwise, you need to ask your network adminstrator
for the appropriate P settngs.
Obtain anIP address automaticaly.
Use the follwing IP address:
1P address: 159115

Subetmask: 255 255 .

Defauit gateway: 159115 .

Obtain DS server address automaticaly
Use the following DS server addresses:
159115

159115

Vaidate settings upon exit
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