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Vehicles
Daphne
· all operations
Other resources
Small Boat
· LRAUV launch & recovery operations
Preparation
Daphne
· expansion coefficient (EC) timeseries for recent past in Data/HFRadarModel on vehicle
· [bookmark: _GoBack]set up an hourly cron job from tellum
Location
· On-shelf -- continuous bottom lock for comparison
· 36.830, -121.870 
· 36.875,-121.967

Mission
Deployment instructions
· Prep vehicle for cart launch and transit via boat and launch within 0.5km of 36.83,-121.87
· Load Engineering/SurfaceCurrentCompactModel.xml and set NeedCommsTime to 20 minutes. 
· Run the mission 
· After first navigation using HF currents, note any dangerous navigation mistakes that could ground the vehicle over the next hour. If noted, issue a stop. 
· Assuming safe navigation, set NeedCommsTime to 60 minutes and run the mission.
· After at least one lap and at a convenient time for operators, transit to 36.83,-121.87 and run Maintenance/ballast_and_trim.xml
· Adjust buoyancy and mass parameters:
· configset VerticalControl.buoyancyNeutral XXX cc persist
· configset VerticalControl.massDefault Y.YYY cm persist
· Continue running SurfaceCurrentCompactModel mission
Post-processing and evaluation
Conclusion

