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Vehicles
Tethys
· all operations
Other resources
Small Boat
· LRAUV launch & recovery operations

Preparation
Tethys
· Short nose standard configuration with Eco Puck and CTD
Location
· Within the box bounded by:
· Latitudes: 36.88 and 36.7
· Longitudes: -122.3 and to within 5km of shore to the East
Mission
· 	Science/canon_2Dfront.xml
Deployment instructions
· Launch vehicle at least 1 km from shore. 
· Run transit mission to 36.82, -121.855 
· Run Maintenance/ballast_and_trim.xml at 50m depth
· Adjust buoyancy and mass parameters:
· configset VerticalControl.buoyancyNeutral XXX cc persist
· configset VerticalControl.massDefault Y.YYY cm persist
· Run Science/canon_2Dfront.xml
· [bookmark: _GoBack]If we have an opportunity to run keepstation in deep water, it would be a good time to test the new buoyancy system at 100 m depth. Be sure to temporarily adjust stop/abort depth settings prior to running. 
Post-processing and evaluation
Conclusion

