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Vehicles
Daphne
· all operations
Other resources
· Paragon for launch & recovery
· MF modem, deck box, and long cable
· GPS position logging to laptop
· Power supply for GPS
Preparation
Daphne
· Long nose with DAT 
Location
· Initially in the vicinity of 36 47.61, -121 50.74
· Then tracking a circle around the Paragon’s motion to the West
Mission
· 	Science/CANON_LST_Track.xml
Deployment instructions
· Launch vehicle near 36 47.61, -121 50.74 (previous LST test site) 
· Deploy topside modem into water at least 15m deep. Make sure address is configured to match ContactLabel
· Activate GPS logging
· Run mission and wait for active tracking (will hear on the topside speaker)
· Move boat slowly or drift allowing AUV to follow

Post-processing and evaluation
· [bookmark: _GoBack]Compare boat position with vehicle position. 

Conclusion

