SCIPI Data Pull

Unplug wet connect or on SCIPI
Plug in test cable
Plug in USB connector (behind 5/8 inch SAE port)
Connect to serial port on laptop
With hyperterm using 9600 N 1 N
Provide 18vdc to power pins on test cable
SCIPI should come up with RDY
 Pwr On to turn on device
Help all for low level commands
[bookmark: _GoBack]Cam on to turn on camera
Plug USB into computer.
When recognized look for files in DCIM directory


