GENOSENSOR TO-DO LIST

June 19, 2000

1. Genosensor

1.1. Camera and brackets (tube length)

Mark




1.2. Arrays





Chris


1.3. Filter holders, o-rings, seals, frits

Mark

1.4. Array printer




Gene

2. Housing





Mark

2.1. Shell







2.2. Mounting legs/arms/brackets




2.3. Bale







2.4. Transport/deployment box




2.5. E/M cable interface cable (both sides)



2.6. External floatation





2.7. Weight and balance spread sheet



3. Mooring





Gene


3.1. Anchor

3.2. Softlines

3.2.1. thimbles

3.3. Chain

3.4. Shackles

3.5. Elastic tethers and brackets

3.6. CTD 





Chris

3.7. CTD bracket

3.8. E/M cable and terminations

3.9. E/M cable floats

3.10. Surface float

3.10.1. Float

3.10.2. Core structure

3.10.3. Antenna tower

3.10.4. Light

3.11. Deployment hardware (line, shackles, blocks, etc.)

3.12. Ship charter

4. Software





Danelle

4.1. Finish testing

4.2. Comm link

4.3. Camera interface

4.4. Long term tests

4.5. Switch ship board and embedded electronics

4.6. Humidity and leak detect circuits

5. Electrical





Scott

5.1. Battery pack

5.1.1. Lead acid 

5.1.2. Charger

5.1.3. Lithium

5.2. Humidity and leak detect circuits

5.3. Telemetry testing

5.3.1. Antenna and cable selection

