4/4/13 Deployment Schedule
Time
Event

0700 
Depart Moss Landing

0800
Arrive on station

0815
Deploy LST 1, for 3 hours hover at 200m

Use pole-mounted transducer to range to LST 1


Range to unit until we are convinced it has stopped it’s descent

0830
Transit a short distance away to begin ROV ops

0845
Deploy ROV, ROV descend to 100 m

0900    Deploy LST 2 for 2 hour hover at 100m
0915 
Locate LST 2 with ROV 


Observe unit and add ballast weight as needed

1000
First burnwire burns, cups rotate

1020
Second burnwire burns, cups rotate

1115
Vehicle ends hover behavior


Send acoustic command to release ascent weight

1120
Carry vehicle to near surface with ROV

1130
Ascent weight burnwire will activate if not acoustically released

1145 
Recover ROV
1215
Recover LST 2


LST1 ends hover, burns ascent weight

1240
Find LST1 and recover from ship
1300
Head back to Moss Landing

