1. ship hull mounted low frequency transducer
a. brett check email

b. cable run from lab to transducer

c. local power and serial?

d. Over-the-side baffled transducer, will be deployed on pole

2. LST

a. Confirm argos goniometer 401.625 MHz

i. needed for recovery of LST

b. Launch and recovery:

i. Launch using pelican hook

ii. how to recover them- use long poly pro line that we try to grapple, need a davit or side-mounted A-frame, spot light on the reflective flag, do we need a stobe
c. Drones

3. Data recovery from the Radar, GPS, Pos MV- real time vs. logged data

a. get everything in the datastream of the reson if possible

4. Phantom deployment and recovery
