1. Servicing of LSTS

1. download data off SOLO

2. download Databridge data

3. replace 3 burnwires

4. service 2 pressure activated guillotines

5. add 2 drop weights

6. flush ctd

7. change out cups

8. program new mission for SOLO and Databridge

9. Run SOLO float built-in test

a. Verify Iridium and GPS working

b. Verify piston pump and air pump working

