LST deployment checklist
1. Preparing the databridge

a. Install shorting plug, tighten locking sleeve

i. Listen for modem to chirp at power up

b. Install Databridge (subconn whip-serial cable) deck cable

c. Open up hyperterminal session, there is probably already one set up labeled “databridge” (settings 9600,8,N,1,N)

d. Pressing enter should bring up databridge menu (if not check shorting plug)

e. Type 5 in the main menu to edit messages

f. Confirm that the message intervals are the desired lengths

g. Once you are happy with intervals double check under ‘recording parameters’ that time stamping is on

h. Return to main menu and type “r” to start recording

i. The main menu should now indicate recording status is on

j. Listen for chirp of modem- this should occur every five minutes

k. Remove databridge deck cable and install dummy plug for deployment

2. Preparing the SOLO Controller

a. Remove SAE plug on top of vehicle and install SOLO deck cable

b. Open hyperterminal (19200,8,N,1,N)

c. Slide magnet across bulls eye

d. If solo does not start up wiggle cable as connection is often tenuous

e. Once you see the solo start to communicate you often must type ‘w’ to wake the controller

f. Once you have reached the main menu follow directions on the SOLO deployment checklist

g. Get GPS fix and check that it has properly set RTC

h. If any parameters are changed do a compute checksum and a verify checksum before deploying

i. When finished remove cable and reinstall plug

3. Preparing the vehicle

a. Make sure CTD plugs are removed

b. Check that all the weights (ascent, descent) are clear
