1. Mob vehicles on the boat at 06:30.
2. transit to site 
3. Deploy first LST

4. use modem to range to vehicle and homer to track it’s descent

5. launch ROV

6. fly ROV to LST

7. LST should hover at 600m (+/- 50m) for 2 hours
8. the open burn wire should start burning immediately and we should inspect to see if the bottles are in the open position.

9. the close burnwire begins burning 1 hour after mission start, and will burn for 45 min

10. if the modem is not commanded from the surface prior the ascent burnwire will start burning after 2 hours. And burn for 45 min

11. the vehicle should start ascending using it’s own buoyancy engine at 2 hrs as well.

12. recover vehicle on surface. Once on surface complete 

