LST setup
1. After vehicle is built up, tested and ready to go

2. Install cup OPEN burnwire
3. 
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4. Install cup Close burnwire
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6. Tie ballast bag on weight drop burn wire, then tie lift line to the same loop, carefully tightening this string until the burnwire is aligned with the lift line.  The extra tension improves the weight drop time.
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