Set up Wan service using web tool. Want to be PPP bridged. 
Under G.SHDSL-> configuration-> make sure Phantom unit is set to remote and top-side is set to Central. Also this will default to a slow speed, the speed should be set to 4608k on both units. 

So far the only way I can find to save the configuration is to telnet to the unit and then use the save command under the configuration menu.

In PPP menu you can enter a new service and see what service is there., you want a brdiged ppp service using hdlc
In gshdsl menu use “set” command to set attributes:

>gshdsl set terminal central (or remote for dsl on phantom)

>

In system menu

>system config save

