December 3, 2008
Do the following to set up the Perle STS4-D:

1. Use the set up wizard to assign a static IP

2. We want the serial ports to be in TRUEPORT mode, this can be set in device manager or web manager once there is an IP

3. Install TruePort software

4. Follow directions in the TruePort Windows User Guide to do Client-Initiated mode (pg8)

5. Make sure in the True port management->Configuration tab->Settings that when you click on the com ports they are set up the following way:

a. Connection mode: Full mode

b. Initiate connection to the device server

c. The TCP port has an address that is 1000+ the port number

READ the following if using PERLE RJ45 to DE9 adapter:

6. Hooking up the Rosetta stone
a. Using the perle RJ45 to DE9 adapter the pin out is as follows

i. Pin 2 Rx

ii. Pin 3 Tx

iii. Pin 8 GND ?#%$^%$

b. To connect to the rosettata stone connect

i. Pin 3 Perle DE9 to Pin 2 on the DE25 of the rosetta

ii. Pin 8 perle de9 to pin 7 on the de25 of the rosetta

iii. Pin 2 Perle De9 to pin 3 on the de25 of the rosetta
7. Hooking up to microCTD

a. Connect ctd DE9 to Perle RJ-45 to DE9 adapter as follows

i. Perle pin 2 to ctd pin 2
ii. Perle pin 3 to ctd pin 3

iii. Perle pin 8 to ctd pin 5

