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Part-Number FM091307-1CP

Foam Polyethylene
0.145" Neon Green

Shiclded Pair, 3:
#24 AWG (1950.005")
tin-plated copper with
polypropylene insulation
rated for 600 opetation
2 cach twisted with flls
60% coverage braid and
AL tape shicld over pair
plus polyethylen jacket
COLOR Cova :

615, 64,544

Polyurethane Jacket
0.049" Neon Green

Kevlar Braid

Inner & Outer Shield:
Drain-wire and AL tape

Power Conductors, 14:
#20 AWG (190.008")
tin-plated copper with
polypropylene insulation

rated for 600v operation
oo cone - bap 0z,

f3, o4, ofs, ofe, /7, 0/3, 0/,

Twisted Quad, 1:
#26 AWG (1950.004")
tin-plated copper with
polypropylene insulation
ated for 600 operation

4 cach twisted together
plus polyethylene jacket O/1/2, /1,912,913
CoLoR cove bower'Conductors,
#24 AWG (19x0.005'
2,2/0,2/4,2/9 tin-plated copper with
950 inch nominal polypropylene insulation
‘Weight in Air = 307 Ibs/1,000 feet nominal rated for 600v operation
Weight in Sea-water = -7 1bs/1,000 fect nominal ~ COLOR cope
Weight in Fr 1bs/1,000 fect nominal 9, /4, /5, /6,
Breaking Strength = 2,000 s nominal
Poak Tension Load = 300 Ibs maximum /7, 9>
Bend Radius = 9 inch minimum
Designed for Ocean Innovations & MBARI
October 19, 2007
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