Sea notes 7 20 2010 BIAUV Barry smooth ridge transectes
· launch at 10:05

· start mission at 10:11

· vehicle headed NW – apparently confused,  sent acoutic aborts though reception was bad; eventually vehicle ascended from 300m
· 11:05 back on surface

· Review of data showed a problem with navigation – appears that by switching the DVL mode from BK1 to BK0 killed navigation.  No water-track, no motion and it didn’t revert to prop RPMs.  Also, there was bad acoustic comms – not sure why.  
· Did a quick spiral mission down to 200m to check comms and tracking – still poor performance

· 11:53 re-started mission and dove

· Decreased mission timmer to 2 hrs to ensure vehicle was back on the surface for a 2:15 recovery

· Spiraled down to 1000m; tracking and A-commms seem OK

· 12: 36  on bottom – issued “start survey” command
· 12:45 started survey

· 1:30 ended survey, issued abort, vehicle spiraled to surface

· 2:15 vehicle recovered

