Cannon camera control software

http://www.breezesys.com/DSLRRemotePro/features.htm
Talks to camera via it’s USB or Firewire port

?can an IP-USB converter be placed between the camera and ethernet?

DSLRRemoteTest.exe
DSLRRemoteTest.exe is a simple command line application that communicates with DSLR Remote Pro and allows the shutter to be released and some of the camera settings to be changed. DSLRRemoteTest.exe and complete source code to build it using Visual C++ .Net can be found in the DSLRRemoteTest folder where DSLR Remote Pro is installed (usually C:\Program Files\BreezeSys\DSLR Remote Pro).

To run DSLRRemoteTest.exe first run DSLR Remote Pro and then open a command prompt window and change directory to the DSLR Remote Pro installation folder. The run DSLRRemoteTest.exe -h to get a list of the available commands.

Here is the output from a simple session where the output directory is set and the shutter is released (commands typed in by the user are shown in bold):

Microsoft Windows XP [Version 5.1.2600]

(C) Copyright 1985-2001 Microsoft Corp.

 

C:\>cd C:\Program Files\BreezeSys\DSLR Remote Pro
 

C:\Program Files\BreezeSys\DSLR Remote Pro>DSLRRemoteTest.exe -h
Usage: DSLRRemoteTest [-w [<shots>] [-i <interval>]] [-a <aperture>] [-s <shutter>]

	 
	-h
	print this usage information

	 
	-w <shots>
	run camera as a webcam for <shots> shots

images are saved as webcam.jpg in the current directory

	 
	-t <interval>
	specify the number of seconds between shots when

used as a webcam

	 
	-a <aperture>
	set the aperture, 0 = widest aperture

	 
	-s <shutter>
	set the shutter speed, 0 = longest shutter speed

	 
	-e <mode>
	set the exposure mode (EOS-1D and EOS-1DS only)

	 
	-x <comp>
	set the exposure compensation

	 
	-i <quality>
	set the image size and quality

	 
	-I <ISO>
	set the ISO

	 
	-c <comment>
	set comment to be added to images (max 255 chars)

	 
	-o <directory>
	set the output directory

	 
	-q
	query output directory

	 
	-n
	don't release shutter


C:\Program Files\BreezeSys\DSLR Remote Pro>DSLRRemoteTest.exe -n -o C:\Photos -q
Output directory: C:\Photos\2004-01-15\

 

C:\Program Files\BreezeSys\DSLR Remote Pro>DSLRRemoteTest.exe
Success, image saved as: C:\Photos\2004-01-15\IMG_0001.JPG

 

C:\Program Files\BreezeSys\DSLR Remote Pro>

