IAUV components
1. D3s
a. Spare is a D3 s#2014034
2. Green Lasers
a. Sidus 10 mW green
3. Lantronics X-port Ethernet to serial adaptor with GPIO
a. Provides an Ethernet socket so the MVC can send:
i. NEMA GPS to Serial port 2 
ii. Release shutter; This uses CP1
iii. Enable 12 Vicor PS; CP2
iv. Toggle relay to enable lasers; CP3
v. [bookmark: _GoBack]Humidity threshold; CP4
vi. 
