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Specifications

	Guide Number (land, ISO 100/m)
	32

	Beam angle
	105°x105°

	Battery
	Battery for YS-250PRO

	Number of flashes
	200

	Recycle time (full)
	1.8

	Color temperature
	5,600K

	Color temperature w/diffuser
	5,200K

	Depth rating
	60m /200ft

	Dimensions (WxHxD)
	107x130x223mm / 4.3x5.2x9inch

	Weight
	1,780g / 62.3oz

	Underwater weight
	-80g / -2.8oz

	Others
	· Exposure control: TTL, Manual(Light-level control)
GN 0.7/1/1.4/2/2.8/4/5.6/8/11/16/22/32 (12 steps) 

· Pre-flash control: Equipped with pre-flash cancel mode (cancels up to two pre-flashes) 

· Slave function 

· Sync cord: Detachable sync cord (N) for film & digital SLR camera,Fiber-optic cable (L-type) for compact digital camera. 

· Over-pressure relief valve 

· LED target light 

· Test flash function 

· TTL confirmation lamp 

· TTL / READY confirmation audible signal


Strobe power

Pulse width

Min


50 usec

1/4


270 usec

3/8


700 usec

1/2


1.1 msec

3/4


3.0 msec

Max


15 msec

