Benthic Imaging AUV
Meeting Minutes – 13 February 2008

1. General

a. Camera system

i. Prosilica is mounted in housing, waiting for electrical harness and P/S installation

ii. Brackets are being fabricated for strobe PCB and P/W mounting

iii. 17” sphere is ready to mount D3

iv. Need a test cable – ethernet – that can penetrate the 17” ball through a 7/16” hole, e.g. Subconn LPBH7M

v. Kent has G-Photo running on his desktop under Lenix and is able to control the Nikon D3.

vi. Kent has the Nikon software talking to the D3 over ethernet

vii. Kent is looking at EXIF to see if we can use for our metadata needs.

viii. Gphoto needs to command different camera settings

ix. Lasers – two down looking

b. AUV

i. Rough layout complete
ii. Need a 30” parallel mid section

iii. Weight and balance needs to be calculated to determine foam 

iv. Task list of refurb is needed

v. New nose cone is due here in a week or two

vi. USBL has been returned from Sonardyne – should be tested.

c. Mission planning

2. Tasks

a. WBS

3. Schedule

a. Ship days: Aug 11, Sept. 11, Nov. 3rd, Nov. 24

b. Milestones: 

i. Lock down Functional Requirements

ii. Demonstrate camera system meets requirements in tank

iii. Lock down initial camera/strobe configuration

iv. Get Camera/strobe under MVC control

v. Demo AUV in Tank

vi. Plan ’09 work – submit proposal

vii. First sea test

viii. First photo mosaic

ix. First science dataset

