Software Requirements
· Control individual chambers, consisting of:

· Stirrer

· CO2 Injector

· O2 Optode

· pH sensor

· Flush pump

· Control via either time-based parameters or ratio of internal to external O2, or a combination of both.  Parameters configurable, presumably by configuration file.  Probably different configuration file than traditional OASIS .cfg file

· Control sets of chambers, where a “set” shares a common flush pump and associated plumbing.

· All chambers in set flushed together, so experiment cycles must be synchronized.

· Any other commonalities (ways to share chamber hardware)?
· Able to add traditional OASIS instrument drivers to the controller serial ports.

· Able to add traditional OASIS drivers to chamber controller serial ports.  Use chamber controller power bits.
