Port Assignments for Dec 1, 2010 BRS Deployment

System Controller
Port 0 – User I/F, RS-232 at 38400 baud
Port 1 – Modbus, RS-485 at 57600 baud
Port 2 – Modbus, RS-485 at 57600 baud

	Chamber controller
	Bus
	ID
	Stir bit/conn
	Inject bit/conn
	Flush bit/conn
	Extract bit/conn
	Optrode serPort/conn
	Connector J3
(serial port 2)

	1
	1
	1
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	

	2
	1
	2
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	

	3
	1
	3
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	

	4
	1
	4
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	Ambient Optrode 

	5
	2
	5
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	

	6
	2
	6
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	

	7
	2
	7
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	

	8
	2
	8
	0 / J4
	2 / J5
	4 / J6
	6 / J7
	1 / J2
	Infrared comm



Chamber Controller 1
Bus 1, ID 1, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2
Chamber Controller 2
Bus 1, ID 2, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2
Chamber Controller 3
Bus 1, ID 3, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2
Chamber Controller 4
Bus 1, ID 4, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Chamber Optrode on serial port 1, connector J2
Ambient Optrode on serial port 2, connector J3
Chamber Controller 5
Bus 2, ID 5, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2



Chamber Controller 6
Bus 2, ID 6, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2
Chamber Controller 7
Bus 2, ID 7, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2
Chamber Controller 8
Bus 2, ID 8, RS-485 at 57600 baud
Stir on bit 0, connector J4
Inject on bit 2, connector J5
Flush on bit 4, connector J6
Extract on bit 6, connector J7
Optrode on serial port 1, connector J2
Infrared User I/F on serial port 2, connector J3


