Respirometer Cheat Sheet
Commands
dp [driver name] – 
display/change driver parameters.  The optional “driver 



name” argument allows you to set the driver parameters of a 


specific driver.

lsample [driver name] – display the most recent sample from a specific driver

modshow – display the modbus networks status

sync [driver name] – cause a pending driver to run immediately

rempulse [output] [seconds] – turn on an output for the specified seconds
Example of Setting “chamber3” Flush Interval
	BRS>

BRS> dp

UserIF               Sampling

stir                 Delay 0.76 secs

optrode1             24 secs

chamber1             Off

optrode2             24 secs

chamber2             Off

optrode3             24 secs

chamber3             Off

optrode4             24 secs

chamber4             Off

optrode5             24 secs

chamber5             Off

optrode6             24 secs

chamber6             Off

optrode7             24 secs

chamber7             Off

optrode8             24 secs

chamber8             Off

optrode9             24 secs

userIR               84 secs

env                  24 secs

BRS>




Continued on next page…

	BRS> dp chamber3
Num  Parameter          Radix Value

  0 Interval (secs)      dec  0  

  1 Serial Port          dec  -1  

  2 Serial Baud Rate     dec  0  

  3 Serial Setup         hex  0  

  4 Power ctrl           hex  0  

  5 Sample type          dec  0  

  6 Hours off mask       hex  0  

  7 Timeout (secs)       dec  1200  

  8 Extra parm 0         dec  0  

  9 Extra parm 1         dec  0  

 10 Extra parm 2         dec  0  

 11 Flags                hex  2  

 12 Counter              dec  0  

Select parm number (0 - 12)  0

Interval (secs)      dec  0  14400

Interval (secs) set to 14400

Select parm number (0 - 12)  

BRS> sync chamber3
BRS> sync chamber3
BRS>










