Layer stack up for Chamber Controller

1.	TOP
2.	GND
3.	PWR
4.	Inner-1
5.	Inner-2
6.	BOT