HSSRT PDR Minutes – Feb 20, 2009

Project Team:

· Dave Caress

· Mark Chaffey

· Rich Henthorn

· Bill Kirkwood

· Paul McGill

Attending:

· Jim Birch

· Mark Brown

· Andy Hamilton

· Kent Headley

· Ed Mellinger

· DJ Osborne

· Keith Raybould

· Brent Roman

· Hans Thomas

Comments:

Acoustic Source

1. Pulse duration spec should be “Minimum pulse duration of 100ms” – Brent

a. OK

2. There should be a “duty-cycle” spec – Hans

a. Agreed

b. Important to heating of xducer and electronics

3. Signal envelope: simple chirp? Hbridge or linear amplifier?

4. What is the cap bank inrush current?

a. Limited by power supply, but must not be shutdown

5. Sound pressure-level spec? – Keith 

a. Louder is better, but is there a minimum? Don’t really know yet

6. Why 1-6kHz sweep?

a. Need 1kHz max lower end, availability, xducer size

b. Signal is 30db down at 1kHz

c. Sweep enables needed time resolution

7. Peter Brewer may have a spare 3000m EdgeTech housing

Acoustic Performance of Receiver 

8. Frequency vs. range?

a. Dunno until we try

9. 15kHz recording frequency

a. Need very good filter to record full bandwidth of source at that recording spec

b. Or, increase the recording frequency to 4-5 times source

10. Need to be tolerant of noise sources like ships, animals

11. Total dynamic range: 16bit digitize (96dB) with a 20 dB gain switch

12. Recorder can record 2 different channels at 2 different gains

a. Phase delay between channels?

b. Can it be done in real-time between pings?

c. Requires firmware mods

d. Is recording SW fast enough?

e. Project not counting on being able to switch gains during experiment

f. May have to accept clipping on near arrivals

13. Direct arrivals used to locate receiver relative to source

14. How omni-directional is the Acousonde?

15. At 300m, there will likely be a significant surface bounce

a. Ping interval should be longer for shallow tests

16. Freq range of receiver ceramic (does it go as low as needed?) - Hans

a. Rolls off less badly than source

b. Spec sheet does not specify that low corner

17. Check spectra from vehicle with simple test

a. Place receivers in sediment, and drive ROV over

b. Piggy-back on another dive

c. EITS collected monotone sound data - DJ

18. Tags are new product

a. Lee Freitag option?

b. B-probe?

c. Packaging – work with DMO

d. Homer-type anchor/float envisioned

e. 0-1m above seafloor

f. Nice to have radar/sonar reflector

g. Place receivers 25-50m apart

Timing Assurance

19. What are pressure, temp, EM effects on oscillator? 

a. Don’t know

b. Will do cold-room test

c. Pressure test?

d. Clock 2ppm over entire temp spec

e. Need 3-4 ppb at constant temp/pressure

f. Characterize performance, then apply correction methods as needed

20. Could we train clock in-situ?

a. Expensive bottom-time testing

21. Does IR work well underwater?

a. Dave Wright had worked with IR in-situ – Bill

22. Why not use IRIG-B?

a. Possibly a better proof-of-concept

b. No need for Phase-lock loop in cRIO

c. Dark fiber availability

d. Simpler, more portable to use serial line

23. Could use time-certain source to provide in-situ background heartbeat - Hans

a. Track receiver clock drift

b. Linksys unit?

