Notes on Designing the Persistor CF2 Prototype for BEDS
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These are some notes on how to interface the various BEDS components to a Persistor CF2.  For the tables below, TPUx means you can use any of the TPU lines, TPU1 through TPU15.
Power
There are two ways to develop power for the Persistor board.  The easiest is to use the on-board linear regulator.  This wastes a lot of battery power, but is very quiet.  A DC-DC converter is more efficient, but may generate too much noise on the Vcc and ground lines for the analog signals.  You just need to try out both.  Talk to Craig Okuda about this (or about anything having to do with the Persistor).  He’s the in-house expert.
If you want to use the on-board linear regulator, just bring the raw battery into CF2 pin 13.  You should add about 10uf of decoupling.  Then tie together CF2 pins 9 and 11, and use that for any 3.3v logic you need.  Again, you should provide about 10uf of decoupling.
If you want to provide a DC-DC converter, leave open pins 11 and 13 on the CF2, and provide 3.3v to CF2 pin 9.  The traditional converter chip to use is the MAX1837EUT33.  But it’s noisy, and possibly not very available any more.  I once did a design with the TPS62125 from TI, but it’s a tiny chip that’s very hard to use. Very efficient, though; and low noise, since it switches at 1 MHz.
Again, talk to Craig Okuda about power for the CF2.  You need to design for a peak current of 200 mA, though the average will be more like 50 or 60 mA.  To that, you need to add whatever current will be used by devices other than the Persistor CF2.
Invensense Chip or Board
This documents the pins on the UC3 proto board from Invensense.  If you want to design directly to the Invensense MPU-6050 chip, just substitute the correct chip pin numbers for the UC3 board pin numbers.
	Persistor CF2
	Invensense UC3 Board

	Pin(s)
	Signal
	Pin(s)
	Signal

	9
	VReg
	10
	3V3_X

	3
	Gnd
	9
	Gnd

	19
	/PCS1
	1
	SDA

	21
	/PCS0
	2
	SCL

	
	TPUx
	8
	PWR_EN_X

	
	TPUx
	
	See note

	40
	/IRQ7
	
	See note


Note – the interrupt signal (MPU_IRQ_X on the UC3 board pin 4) needs to be conditioned and sent to /IRQ7 on the CF2.  But it needs to be NAND’ed with a TPU bit.  Bring the MPU_IRQ_X and any TPU line into a NAND gate, and send the output to /IRQ7.  The TPU line needs a weak (1M) pull-down to ground.
Clock Chip – Maxim DS3234
	Persistor CF2
	Maxim 3234

	Pin(s)
	Signal
	Pin(s)
	Signal

	15
	/PCS2
	1
	/CS

	16
	SCK
	20
	SCK

	18
	MOSI
	17
	DIN

	20
	MISO
	19
	DOUT

	14
	Vbbk
	16
	Vbat

	41
	/IRQ2
	5
	/Int

	
	
	3
	32kHz - note


Note – Bring pin 3 to a test point on the board

ADS8344 Analog-Digital Converter
	Persistor CF2
	ADS8344

	Pin(s)
	Signal
	Pin(s)
	Signal

	17
	/PCS3
	18
	/CS

	16
	SCK
	19
	SCK

	18
	MOSI
	17
	DIN

	20
	MISO
	15
	DOUT

	
	TPUx
	10
	/SHDN


Note – Pin 11, Vref, should be connected to a LT1461 reference.  The TPU line driving /SHDN should also drive the Shutdown pin of the LT1461.  Just copy the design on page 13 of the ReceipeCards data sheet.

Serial Ports
The main serial console port should be pinned out as shown on page 13 of the RecipeCards data sheet.  In addition, we’ll need a serial port for the acoustic modem.  Pick two TPU lines for Rx and Tx.  Traditionally, it would be TPU15 and 14, or TPU13 and 12.  But any two will do.  Wire them into an RS-232 driver chip, e.g. the MAX3222, as shown on the RecipeCards data sheet.  Bring the EIA signals out to a connector you deem appropriate for wiring to the modem.

Miscellaneous
Please also wire the WAKE, PBM, and RESet pushbuttons as shown on the RecipeCards data sheet.  Also the Lithium backup battery, which is critical to proper operation.  We don’t need the LEDs.

