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This is a list of variables that affect the operation of BEDS.  The intent is that these variables can be set by either a configuration file (BEDS.CFG) or via a user interface command.
	Variable Name
	Default
	Use

	EvtFreq
	50
	FIFO rate during event, = freq of INU records during event

	WatchFreq
	10
	FIFO rate durint watch mode

	LowBattNoSample
	
	Low battery voltage at which we stop getting INU data

	LowBattOff
	
	Low battery voltage at which we turn off entire system

	ModemPeriod
	3600
	Period (secs) for turning on acoustic modem

	ModemOnTime
	60
	Period we leave modem on

	AccelRange
	16
	Accelerometer range in g’s

	GyroRange
	2000
	Gyro range in degrees/sec

	DigitalFilterBW
	42
	Bandwidth of digital filter on MPU6000.  Allowable values are 5, 10, 20, 42, 98, 188 or 256 Hz.  Will set to next lower value.

	NoMotionThresh
	
	MPU no motion threshold

	NoMotionTime
	
	MPU no motion time

	BEDSLogLevel
	
	Log level for the BEDS software

	InvLogLevel
	
	Log level for the Invensense stack logging routines



