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This is a list of the BEDS operating variables.  All variables on this list can be changed in two ways:
1. Via the user interface.  The following commands are equivalent.  Commands are case-insensitive (capitalization doesn’t matter), but you must have a space before and after the = sign.
accelRange  =  16
var accelRange 16
At startup via the BEDS.CFG configuration file.  Only the name = value form works:
accelRange = 16
	Variable Name
	Units
	Dflt
	Type
	Min
	Max
	Use

	PlatformID
	
	0
	I
	1
	10^9
	Platform ID that is put into data files

	DeploymentID
	
	0
	I
	1
	10^9
	Unique ID for deployment, starting at 0

	ModemAddr
	
	1
	I
	1
	99
	Address to initialize modem with (S18)
Note this may be different from PlatformID

	EvtFreq
	Hz
	50
	I
	10
	1000
	Sample rate during event, = freq of INU records during event

	WatchFreq
	Hz
	10
	I
	1
	100
	Sample rate during watch mode

	ModemPeriod
	Secs
	3600
	I
	300
	7200
	Period (secs) for turning on acoustic modem

	DeployModemPeriod
	Secs
	600
	I
	120
	1800
	Modem period during deployment mode

	DeployModeSecs
	Secs
	86400
	I
	3600
	1 week
	Amount of time to stay in deployment mode

	ModemOffset
	Secs
	0
	I
	0
	3600
	See note (2)

	ModemOnTime
	Secs
	60
	I
	60
	3600
	Period we leave modem on, seconds

	ModemWarmup
	Secs
	15
	I
	5
	600
	Time after modem powerup to wait for signon message, before watching for actual characters from topside

	ModemWait
	Secs
	5
	I
	1
	120
	Time to wait before turning off modem, to allow all serial traffic to reach the topside modem

	ModemPower
	Level
	6
	I
	2
	8
	S6 setting (Tx power) for modem

	AccelRange
	g
	16
	I
	2
	16
	Accelerometer range in g’s.  Valid values: 2, 4, 8, or 16

	GyroRange
	deg/s
	2000
	I
	250
	2000
	Gyro range in deg/sec. Valid values: 250, 500, 1000, 2000

	DigitalFilterBW
	Hz
	42
	I
	5
	256
	Bandwidth of digital filter on MPU6000.  Allowable values are 5, 10, 20, 42, 98, 188 or 256 Hz.  Will set to next lower value.

	Timeout
	Secs
	120
	I
	60
	3600
	Timeout on user I/F, seconds

	MaxEvent
	Secs
	7200
	I
	1800
	43200
	Max length of recorded event, seconds

	EventPressureSecs
	Secs
	1
	I
	1
	600
	Period for sampling pressure during an event, seconds

	SysRecSecs
	Secs
	600
	I
	1
	3600
	Period for sampling system  parameters during watch cycle

	NoMotionThresh
	Deg/s
	2.0
	F
	*
	*
	MPU no motion threshold in gyro degrees/sec 

	NoMotionTime
	Secs
	2.0
	F
	*
	*
	MPU no motion time, seconds

	SensorWarmup
	Secs
	5
	I
	2
	60
	Power-on warmup before sampling system sensors, secs

	SensorMinSecs
	Secs
	5
	I
	2
	60
	If SysRecSecs < this, leave sensors on

	ModemBaud
	Bits/s
	9600
	I
	300
	115200
	Baud rate to talk to acoustic modem

	DebugBaud
	Bits/s
	9600
	I
	300
	115200
	Baud rate to talk to aux serial port (debug port)

	kermitTimeout
	Secs
	30
	
	10
	300
	Timeout for Kermit protocol

	Echo
	Bool
	TRUE
	B
	*
	*
	Echo user commands when using acoustic modem

	InitModem
	Bool
	TRUE
	B
	*
	*
	TRUE to send init strings to modem at boot

	InitPicoClock
	Bool
	TRUE
	B
	*
	*
	TRUE to init PicoDOS clock from RTC at boot

	logToConsole
	
	0
	I
	0
	3
	See note (3)

	zmSetRemote
	Bool
	TRUE
	B
	*
	*
	Deployed side attempts to set top side S Registers during ZModem transfer



Type Field consists of one or more of the following:
I – Integer (32 bit)
F – Float (32 bit)
S – String variable (32 chars max)
B – Boolean (TRUE or FALSE)
Notes
(*)  Min/max only enforced for integer (32 bit) variables
(1) Currently not used.
(2) – Normally, we will power the modem on an even boundary of ModemPeriod.  E.g., for ModemPeriod=3600, we will start on the hour.  ModemOffset allows you to offset that convention by a given number of seconds.  In the above example, if ModeOffset is 300 seconds, the modem will be powered starting at 5 minutes after the hour.
 (3) Normally, significant events are logged to the system log file SYSLOG.TXT.  This variable will also output those messages to one of the serial ports, as follows:
  0 – Normal operation, don’t echo to serial port
  1 – Also echo to the main system console serial port
  2 – Echo to the aux (debug) serial port
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There is one additional variable that can be set in BEDS.CFG, though not in the user interface.  This is because by the time the user interface runs, it’s too late.  That variable is 
START – set system to start after a delay from initial power-up, or at a specified time.  There are two forms:
START AFTER <n>[s|m|h|d]
This will start the system with a fixed delay after the power-plug is inserted.  With no trailing character, it’s specified in seconds.  The trailing character modifies this to be minutes (m), hours (h), or days (d).  For example START AFTER 6h will start the system with a delay of 6 hours.
START [mm/dd/yyyyThh:mm:ss]
This starts the system at the absolute time specified.  Note the ‘T’ that separates the date from the time.  This can be any character, but must be non-blank.  Other notes on this form:
· If the date is specified without the time, it will start at 00:00:00 on the specified date
· If the time is specified without the date, it will start at time hh:mm:ss of the current day.  Be careful – if the time has passed, the system starts immediately.
· The date can be specified as simply mm/dd.  The system assumes the current year.  Be careful – if the date has passed, the system starts immediately.
· The time can be specified as simply hh:mm.  This is equivalent to hh:mm:00

