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Purpose
The BEDS system will have both a direct serial port for system development, debugging, and calibration in the lab, as well as an acoustic modem to allow us to contact the system acoustically while it is deployed.  In both cases, we need a simple character based (command-line driven) user interface to allow us to examine and modify the system, and to download data.
System Facilities
BEDS is designed around a Persistor CF2 microcontroller.   The CF2 has a built-in operating system called PicoDOS, which was designed to look like MS-DOS.  It has a command-line processor, as well as many built-in commands that mimic DOS commands.  It is assumed that the user will be familiar with these standard DOS commands.
In addition to the standard PicoDOS commands, we will add a number of BEDS-specific commands.  Those are documented in the “BEDS Commands” section.  The PicoDOS commands are summarized in the “PicoDOS Commands” section, but not as thoroughly documented.  Both the BEDS commands and PicoDOS commands are always available at the command line.
Design note – It is possible to delete any PicoDOS commands that are deemed too dangerous to include in a deployed system.  We should discuss what commands should be deleted.
BEDS Commands
In Progress…
Events Command
Syntax
Events 
GetEvent Command
Syntax
GetEvent 


PicoDOS Commands
(Many need to be deleted, but here they all are…)
APP
ATTRIB
BACKROM
BOOT
CAPTURE
CCC
CHDIR
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COPY
DUMP
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RMDIR
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SET
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