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Purpose

Multibeam mapping of Monterey Canyon has revealed the existence of crescent-shaped bedforms in the axial channel extending from the canyon head (~11 m) down to ~1900 m water depth. AUV multibeam mapping surveys of other submarine canyons along the California continental margin show that these features are characteristic of active submarine canyons. The occurrence of these bedforms has captured the attention of the marine geologic community and the origin of these features is already controversial.

Our recent efforts to determine the origin of these bedforms have included monitoring the movement of buried homer beacons, repeated AUV-multibeam mapping surveys, and ROV vibracoring in upper Monterey Canyon. Results obtained so far have clearly demonstrated that the bedforms are generated during brief, energetic sediment transport events that occur a few times each year, which are capable of moving boulder-sized objects hundreds of meters down-canyon. 

What actually happens in these sediment transport events is less clear. The initial assumption, which logically extended from the existing paradigm, was that the wave-like bedforms are produced by suspension and redeposition of sediments during high-energy turbidity events. In contrast, our data suggest that large sections of the canyon floor appear to move in a slump-like fashion during these events, somewhat analogous to movement of ice within a glacier. This new model challenges the turbidity current model and forces us to re-interpret old data and assumptions. At issue is whether the sediment transport events are turbidity currents that exhume material from the canyon floor and carry it either suspended in the water column, as bedload over the seafloor before it is redeposited further down canyon, or as down-canyon translations of large coherent segments of the seafloor. The depth to which the bottom movements penetrate is unknown, but sustained translation of the seafloor down-canyon is a potential mechanism for carving the canyon into its host rock. An instrument buried in the seafloor designed to record motion during the down-canyon sediment movement would aid in discriminating between the turbidity current, bedload, or coherent-slab transport models.

Methods and Equipment

We are developing a Benthic Event Detector (BED) to measure the down-canyon movement of the sediments within Monterey Canyon during mass transport events. This project will determine the feasibility of constructing a self-contained sensor system (the BED) that detects seafloor sediment motion.
The BED is equipped with an integrated suite of motion sensors, a pressure transducer, acoustic modem, and acoustic transducer. It will be buried just below the sediment surface. This unique sensor will aid in evaluating the new hypothesis that sedimentary fill within submarine canyon floors may move downslope as large masses, not primarily in suspension in the water column above the seafloor or as bedload moving over the surface of the seafloor. If it is conclusively demonstrated that substantial sub seafloor movements are occurring, this promises to overturn existing paradigms that explain how sediment moves down submarine canyons.

Sanctuary Prohibitions

There will be minor seafloor alterations at the deployment sites. Because these devices will move during sediment transport events, these alterations will be “erased” during such events. All equipment will be recovered at the end of the experiment.

Sanctuary Activities in 2012
None 
Plans for 2013
Activities in 2013 involve a prototype instrument deployment to evaluate initial motion measurements.
Prototype BED Testing in Upper Monterey Canyon: Up to six prototype BEDs (18 inches diameter; approximately 45 lbs in air) with an attached acoustic transponder will be deployed in upper Monterey Canyon in approximately 100-300 meters water depth in mid-April. This BED prototype deployment will obtain some basic sediment movement data that is essential for better defining the requirements of the instrument package. This prototype will be placed on the seafloor, and the location, tracking, and communication tests and ultimate recovery will occur over a period of approximately 8 months. Recovery is scheduled for December 12, 2013 via the R/V Rachel Carson and the ROV Ventana. 
Plans for 2013 and beyond

The project team hopes to deploy multiple BED instruments in 2014 in conjunction with other event detection monitoring systems, including STEDs and McSTAR (see project #901023 for additional details on these systems). If this integrated experiment proves successful, the team will work to integrate data from all three systems and deploy additional systems in future years.
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