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Mother Board Rev2 Wish List, high-to-low priority: 
1. Fix coin cell polarity & new (more reliable) coin cell holder  - YES
2. Internal monitoring of 3.3v coin cell voltage – TEST CONNECTOR
3. Load test for Pack 1, Pack 2, reporting voltage at ~ 1mA load – TEST CONNECTOR
4. Interface for Density Sensor?  - NO 
5. New mechanical and electrical interface for a new gen sensor board? – NO 
6. Audio buzzer on Mother Board; Audio conformation of event triggering; Audio conformation of flowchart transitions – NO 
7. Interface to self-tester: small motor to vibrate board? NO 
8. Interface to proximity sensor? – NO 
9. Bluetooth interface on the 2nd serial port,
with a power switch to turn it on/off.  We could leave it on for 24 hours during
"deploy" mode, then power cycle it at very low duty cycle.  Perhaps add a "recovery"
mode to again leave it on.  It allow us to make last minute changes during deployment and give us a way to recover data from a recovered can without opening the can.

Other improvements: 

1. Pressure sensor to avoid corrosion 

2. Revise mechanics 

