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Hi Denis and Brian,
[bookmark: _GoBack]
I have the BEDS topside modem! Sorry, didn't know you were looking. 
Denis and I did some debugging in the lab. These are my notes. 

Summary:
Denis:
    * Try different SD card
    * 115200 on J8

Elecia:
    * Hot swap of serial port seems to cause drive issue
    * Look at modem output on J7

More detail:
The drive on the lab BEDS unit is not working. It seems to have degraded over time. Can you put in a new SD card?
You can bring it here and I can put in a new SD card and verify it works but if a new SD works, I'm just going to throw the old one away so if you have an another drive, no need to bring it over. 

Linear motion doesn't have a threshold, only rotational. To get events on the linear motion change the threshold variable variable:
var NoMotionThresh = 0.5
(the default is var NoMotionThresh = 2.0, you may want to put it somewhere between 0.5 and 2.0 as 0.5 seems too sensitive)

BUG for me to look at: it seems to be wiping memory on hot swap of the serial port. Try this. In the short term, power down before swapping serial port. Please let me know if the memory gets wiped without a serial port hot swap (so I stop looking at the serial hot swap and look more at power down). 

For Denis to look at: Try a more modern computer to connect 115200 on J8. This is the one I use. It will talk anytime (but J7 is 9600 baud and only talks every 10 minutes unless you reset.

After a reset:
priv 100
var NoMotionThresh = 0.5
deploy -N
imucal
    Needs to have the gyro calibration set to 3

To send a file
priv 100
yr 
    Y-Modem Receive for BEDS.CFG file, send in HyperTerm

Let's meet again Friday at 3pm over Zoom.

Thanks,
Elecia
